Help

# Status / Tuner tab

The Status / Tuner tab (Pic 20) displays various reception parameters. Changes of the parameters become effective after the Apply button (Pic 1) has been pressed.

Pic 20, Tuner status, and tuner settings

## Tuner status

### Synchronization

The box indicates whether a DVB signal has been detected.

### Signal quality

Indicates the quality of the received signal. A value of 100% indicates a faultless reception (Bit error rate less than 10-4).

### Signal level

The level of the received signal in percentage terms.

## Tuner settings

### Frequency

This allows you to set the
.
The
can either be entered manually or gradually adjusted using the arrow keys.

###