Help: Channel Scan

# Channel Scan

The dialog-window Channel Scan provides Services to seek new DVB-Stations and/or actualize the Programme list.
Use the Button Cancel to close the Window Channel Scan and return to the main-window. Changes that have been made in the Programme list will not be saved.
OK also closes the dialog-window, but saves new oder edited channels in the Programme list.

## Programme list

### List

Listing of the current Programme list.
Already existing channels are displayed blue. In contrast to new channels, which are displayed red and updated channels that are green-coloured. One or more channels can be marked. Scrambled Channels are labeled by a rhomb (#).
Below the Programme list the amount of New/Updated and Total-Channels for TV and Radio is shown.

### TV / Radio

Choose, whether TV or Radio-Channels should be shown.

### New only

Activate this button, if you want to see the new channels only.

### Updated only

Activate this button, if you want to see the updated channels only.

### Remove all

Press this button, to remove all channels.

Hint: To remove a single channel, mark it an press DEL.

### Sort

You can sort the Programme list by clicking the appropriate columnheader.

## Signal status

Lock: | Indicates, whether a DVB-Transponder was found or not.
Level: | Shows the SNR (Signal-Noise-Ratio) of the locked signal.
Quality: | Displays the Bit-Error-Rate in 4 Steps (better than 10-1, 10-2, 10-3 or 10-4).

## Scanning status

Displays the current adjusted satelite and the actual frequency and signal-state, while the channelscan is running.

## LNB/Satelite

Repertory of the LNB respective the satelite, where you want to scan and update channels.

## Progress

The appropriate channelnumber, frequency and symbolrate are displayed while scanning automatically.

## Automatic Scan

Start the automatic fast channelscan by clicking this button. The whole frequency-range (based on the transponder-table) on the selected satelite will be scanned.